#MicroXplorer Configuration settings - do not modify
CAN1.ABOM=ENABLE
CAN1.BS1=CAN_BS1_14TQ
CAN1.BS2=CAN_BS2_3TQ
CAN1.CalculateBaudRate=500000
CAN1.CalculateTimeBit=1999.99
CAN1.CalculateTimeQuantum=111.11111111111111
CAN1.IPParameters=CalculateTimeQuantum,CalculateTimeBit,CalculateBaudRate,ABOM,NART,Prescaler,BS1,BS2,SJW
CAN1.NART=ENABLE
CAN1.Prescaler=5
CAN1.SJW=CAN_SJW_2TQ
FMC.AddressSetupTime1=3
FMC.BusTurnAroundDuration1=1
FMC.CASLatency1=FMC_SDRAM_CAS_LATENCY_3
FMC.CASLatency2=FMC_SDRAM_CAS_LATENCY_3
FMC.ColumnBitsNumber1=FMC_SDRAM_COLUMN_BITS_NUM_9
FMC.ColumnBitsNumber2=FMC_SDRAM_COLUMN_BITS_NUM_9
FMC.DataSetupTime1=3
FMC.ExitSelfRefreshDelay1=8
FMC.ExitSelfRefreshDelay2=8
FMC.IPParameters=WriteOperation1,AddressSetupTime1,DataSetupTime1,BusTurnAroundDuration1,ColumnBitsNumber1,CASLatency1,SDClockPeriod1,SDClockPeriod2,ReadBurst1,ReadBurst2,ReadPipeDelay1,ReadPipeDelay2,LoadToActiveDelay1,ExitSelfRefreshDelay1,SelfRefreshTime1,RowCycleDelay1,RowCycleDelay2,WriteRecoveryTime1,RPDelay1,RPDelay2,RCDDelay1,WriteRecoveryTime2,ExitSelfRefreshDelay2,ColumnBitsNumber2,CASLatency2,LoadToActiveDelay2,SelfRefreshTime2,RCDDelay2
FMC.LoadToActiveDelay1=2
FMC.LoadToActiveDelay2=2
FMC.RCDDelay1=2
FMC.RCDDelay2=2
FMC.RPDelay1=2
FMC.RPDelay2=2
FMC.ReadBurst1=FMC_SDRAM_RBURST_ENABLE
FMC.ReadBurst2=FMC_SDRAM_RBURST_ENABLE
FMC.ReadPipeDelay1=FMC_SDRAM_RPIPE_DELAY_1
FMC.ReadPipeDelay2=FMC_SDRAM_RPIPE_DELAY_1
FMC.RowCycleDelay1=6
FMC.RowCycleDelay2=6
FMC.SDClockPeriod1=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SDClockPeriod2=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SelfRefreshTime1=6
FMC.SelfRefreshTime2=6
FMC.WriteOperation1=FMC_WRITE_OPERATION_ENABLE
FMC.WriteRecoveryTime1=4
FMC.WriteRecoveryTime2=4
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.Family=STM32F4
Mcu.IP0=CAN1
Mcu.IP1=FMC
Mcu.IP10=TIM10
Mcu.IP11=TIM11
Mcu.IP12=TIM12
Mcu.IP13=TIM13
Mcu.IP14=TIM14
Mcu.IP15=USART1
Mcu.IP16=USART6
Mcu.IP2=NVIC
Mcu.IP3=RCC
Mcu.IP4=SPI1
Mcu.IP5=SPI2
Mcu.IP6=SPI3
Mcu.IP7=SYS
Mcu.IP8=TIM8
Mcu.IP9=TIM9
Mcu.IPNb=17
Mcu.Name=STM32F446Z(C-E)Tx
Mcu.Package=LQFP144
Mcu.Pin0=PC13
Mcu.Pin1=PC14-OSC32_IN
Mcu.Pin10=PH1-OSC_OUT
Mcu.Pin11=PC0
Mcu.Pin12=PC3
Mcu.Pin13=PA4
Mcu.Pin14=PA6
Mcu.Pin15=PA7
Mcu.Pin16=PC4
Mcu.Pin17=PF11
Mcu.Pin18=PF12
Mcu.Pin19=PF13
Mcu.Pin2=PC15-OSC32_OUT
Mcu.Pin20=PF14
Mcu.Pin21=PF15
Mcu.Pin22=PG0
Mcu.Pin23=PG1
Mcu.Pin24=PE7
Mcu.Pin25=PE8
Mcu.Pin26=PE9
Mcu.Pin27=PE10
Mcu.Pin28=PE11
Mcu.Pin29=PE12
Mcu.Pin3=PF0
Mcu.Pin30=PE13
Mcu.Pin31=PE14
Mcu.Pin32=PE15
Mcu.Pin33=PB12
Mcu.Pin34=PB13
Mcu.Pin35=PB14
Mcu.Pin36=PB15
Mcu.Pin37=PD8
Mcu.Pin38=PD9
Mcu.Pin39=PD10
Mcu.Pin4=PF1
Mcu.Pin40=PD14
Mcu.Pin41=PD15
Mcu.Pin42=PG2
Mcu.Pin43=PG4
Mcu.Pin44=PG5
Mcu.Pin45=PG8
Mcu.Pin46=PC6
Mcu.Pin47=PC7
Mcu.Pin48=PC8
Mcu.Pin49=PA9
Mcu.Pin5=PF2
Mcu.Pin50=PA10
Mcu.Pin51=PA13
Mcu.Pin52=PA14
Mcu.Pin53=PA15
Mcu.Pin54=PC10
Mcu.Pin55=PC12
Mcu.Pin56=PD0
Mcu.Pin57=PD1
Mcu.Pin58=PD4
Mcu.Pin59=PD5
Mcu.Pin6=PF3
Mcu.Pin60=PD6
Mcu.Pin61=PD7
Mcu.Pin62=PG15
Mcu.Pin63=PB3
Mcu.Pin64=PB4
Mcu.Pin65=PB5
Mcu.Pin66=PB6
Mcu.Pin67=PB8
Mcu.Pin68=PB9
Mcu.Pin69=PE0
Mcu.Pin7=PF4
Mcu.Pin70=PE1
Mcu.Pin71=VP_SYS_VS_Systick
Mcu.Pin72=VP_TIM8_VS_ClockSourceINT
Mcu.Pin73=VP_TIM9_VS_ClockSourceINT
Mcu.Pin74=VP_TIM10_VS_ClockSourceINT
Mcu.Pin75=VP_TIM11_VS_ClockSourceINT
Mcu.Pin76=VP_TIM12_VS_ClockSourceINT
Mcu.Pin77=VP_TIM13_VS_ClockSourceINT
Mcu.Pin78=VP_TIM14_VS_ClockSourceINT
Mcu.Pin8=PF5
Mcu.Pin9=PH0-OSC_IN
Mcu.PinsNb=79
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F446ZETx
MxCube.Version=6.1.0
MxDb.Version=DB.6.0.10
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.CAN1_RX0_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.CAN1_TX_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.EXTI15_10_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.EXTI9_5_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.TIM1_BRK_TIM9_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.TIM1_TRG_COM_TIM11_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.TIM1_UP_TIM10_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.TIM8_BRK_TIM12_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.TIM8_TRG_COM_TIM14_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.TIM8_UP_TIM13_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.USART1_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.USART6_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA15.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PA15.GPIO_Label=SPI3_NSS
PA15.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA15.GPIO_PuPd=GPIO_PULLUP
PA15.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA15.Locked=true
PA15.PinState=GPIO_PIN_SET
PA15.Signal=GPIO_Output
PA4.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PA4.GPIO_Label=SPI1_NSS
PA4.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA4.GPIO_PuPd=GPIO_PULLUP
PA4.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA4.Locked=true
PA4.PinState=GPIO_PIN_SET
PA4.Signal=GPIO_Output
PA6.Locked=true
PA6.Mode=Full_Duplex_Master
PA6.Signal=SPI1_MISO
PA7.Locked=true
PA7.Mode=Full_Duplex_Master
PA7.Signal=SPI1_MOSI
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB12.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PB12.GPIO_Label=SPI2_NSS
PB12.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PB12.GPIO_PuPd=GPIO_PULLUP
PB12.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PB12.Locked=true
PB12.PinState=GPIO_PIN_SET
PB12.Signal=GPIO_Output
PB13.Locked=true
PB13.Mode=Full_Duplex_Master
PB13.Signal=SPI2_SCK
PB14.Locked=true
PB14.Mode=Full_Duplex_Master
PB14.Signal=SPI2_MISO
PB15.Locked=true
PB15.Mode=Full_Duplex_Master
PB15.Signal=SPI2_MOSI
PB3.Locked=true
PB3.Mode=Full_Duplex_Master
PB3.Signal=SPI1_SCK
PB4.Locked=true
PB4.Mode=Full_Duplex_Master
PB4.Signal=SPI3_MISO
PB5.Locked=true
PB5.Mode=SdramChipSelect2_2
PB5.Signal=FMC_SDCKE1
PB6.Locked=true
PB6.Mode=SdramChipSelect2_2
PB6.Signal=FMC_SDNE1
PB8.Locked=true
PB8.Mode=CAN_Activate
PB8.Signal=CAN1_RX
PB9.Locked=true
PB9.Mode=CAN_Activate
PB9.Signal=CAN1_TX
PC0.Signal=FMC_SDNWE
PC10.Locked=true
PC10.Mode=Full_Duplex_Master
PC10.Signal=SPI3_SCK
PC12.Locked=true
PC12.Mode=Full_Duplex_Master
PC12.Signal=SPI3_MOSI
PC13.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PC13.GPIO_Label=LED
PC13.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PC13.GPIO_PuPd=GPIO_PULLUP
PC13.Locked=true
PC13.PinState=GPIO_PIN_SET
PC13.Signal=GPIO_Output
PC14-OSC32_IN.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label
PC14-OSC32_IN.GPIO_Label=W5500_RST
PC14-OSC32_IN.GPIO_PuPd=GPIO_PULLUP
PC14-OSC32_IN.Locked=true
PC14-OSC32_IN.PinState=GPIO_PIN_SET
PC14-OSC32_IN.Signal=GPIO_Output
PC15-OSC32_OUT.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PC15-OSC32_OUT.GPIO_Label=W5500_INT
PC15-OSC32_OUT.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PC15-OSC32_OUT.GPIO_PuPd=GPIO_PULLUP
PC15-OSC32_OUT.Locked=true
PC15-OSC32_OUT.Signal=GPXTI15
PC3.Mode=SdramChipSelect1_1
PC3.Signal=FMC_SDCKE0
PC4.Locked=true
PC4.Mode=SdramChipSelect1_1
PC4.Signal=FMC_SDNE0
PC6.Mode=Asynchronous
PC6.Signal=USART6_TX
PC7.Mode=Asynchronous
PC7.Signal=USART6_RX
PC8.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PC8.GPIO_Label=USART6_EN
PC8.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_PP
PC8.GPIO_PuPd=GPIO_PULLDOWN
PC8.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PC8.Locked=true
PC8.PinState=GPIO_PIN_RESET
PC8.Signal=GPIO_Output
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD4.Signal=FMC_NOE
PD5.Signal=FMC_NWE
PD6.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PD6.GPIO_Label=FPGA_12K_INT
PD6.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PD6.GPIO_PuPd=GPIO_PULLUP
PD6.Locked=true
PD6.Signal=GPXTI6
PD7.Mode=NorPsramChipSelect1_1
PD7.Signal=FMC_NE1
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF11.Signal=FMC_SDNRAS
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG15.Signal=FMC_SDNCAS
PG2.Signal=FMC_A12
PG4.Signal=FMC_A14_BA0
PG5.Signal=FMC_A15_BA1
PG8.Signal=FMC_SDCLK
PH0-OSC_IN.Mode=HSE-External-Clock-Source
PH0-OSC_IN.Signal=RCC_OSC_IN
PH1-OSC_OUT.Mode=HSE-External-Clock-Source
PH1-OSC_OUT.Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=270
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F446ZETx
ProjectManager.FirmwarePackage=STM32Cube FW_F4 V1.25.2
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=EMBOS.ioc
ProjectManager.ProjectName=EMBOS
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-LL-true,2-SystemClock_Config-RCC-false-LL-false,3-MX_USART1_UART_Init-USART1-false-LL-true,4-MX_USART6_UART_Init-USART6-false-LL-true,5-MX_FMC_Init-FMC-false-HAL-true,6-MX_SPI1_Init-SPI1-false-LL-true,7-MX_CAN1_Init-CAN1-false-HAL-true,8-MX_SPI2_Init-SPI2-false-LL-true,9-MX_SPI3_Init-SPI3-false-LL-true,10-MX_TIM8_Init-TIM8-false-LL-true,11-MX_TIM9_Init-TIM9-false-LL-true,12-MX_TIM10_Init-TIM10-false-LL-true,13-MX_TIM11_Init-TIM11-false-LL-true,14-MX_TIM12_Init-TIM12-false-LL-true,15-MX_TIM13_Init-TIM13-false-LL-true,16-MX_TIM14_Init-TIM14-false-LL-true
RCC.AHBFreq_Value=180000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=45000000
RCC.APB1TimFreq_Value=90000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=90000000
RCC.APB2TimFreq_Value=180000000
RCC.CECFreq_Value=32786.88524590164
RCC.CortexFreq_Value=180000000
RCC.FCLKCortexFreq_Value=180000000
RCC.FMPI2C1Freq_Value=45000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=180000000
RCC.HSE_VALUE=12000000
RCC.I2S1Freq_Value=96000000
RCC.I2S2Freq_Value=96000000
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CECFreq_Value,CortexFreq_Value,FCLKCortexFreq_Value,FMPI2C1Freq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,I2S1Freq_Value,I2S2Freq_Value,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLI2SM,PLLI2SPCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SoutputFreq_Value,PLLM,PLLN,PLLQCLKFreq_Value,PLLRCLKFreq_Value,PLLSAIM,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIoutputFreq_Value,PLLSourceVirtual,PWRFreq_Value,PWR_Regulator_Voltage_Scale,SAIAFreq_Value,SAIBFreq_Value,SDIOFreq_Value,SPDIFRXFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,USBFreq_Value,VCOI2SInputFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIInputFreq_Value,VCOSAIOutputFreq_Value
RCC.MCO2PinFreq_Value=180000000
RCC.PLLCLKFreq_Value=180000000
RCC.PLLI2SM=12
RCC.PLLI2SPCLKFreq_Value=96000000
RCC.PLLI2SQCLKFreq_Value=96000000
RCC.PLLI2SRCLKFreq_Value=96000000
RCC.PLLI2SoutputFreq_Value=96000000
RCC.PLLM=12
RCC.PLLN=360
RCC.PLLQCLKFreq_Value=180000000
RCC.PLLRCLKFreq_Value=180000000
RCC.PLLSAIM=12
RCC.PLLSAIPCLKFreq_Value=96000000
RCC.PLLSAIQCLKFreq_Value=96000000
RCC.PLLSAIoutputFreq_Value=96000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWRFreq_Value=180000000
RCC.PWR_Regulator_Voltage_Scale=PWR_REGULATOR_VOLTAGE_SCALE1
RCC.SAIAFreq_Value=96000000
RCC.SAIBFreq_Value=96000000
RCC.SDIOFreq_Value=180000000
RCC.SPDIFRXFreq_Value=180000000
RCC.SYSCLKFreq_VALUE=180000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLRCLK
RCC.USBFreq_Value=180000000
RCC.VCOI2SInputFreq_Value=1000000
RCC.VCOI2SOutputFreq_Value=192000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=360000000
RCC.VCOSAIInputFreq_Value=1000000
RCC.VCOSAIOutputFreq_Value=192000000
SH.FMC_A0.0=FMC_A0,13b-a1
SH.FMC_A0.1=FMC_A0,13b-sda1
SH.FMC_A0.2=FMC_A0,13b-sda2
SH.FMC_A0.ConfNb=3
SH.FMC_A1.0=FMC_A1,13b-a1
SH.FMC_A1.1=FMC_A1,13b-sda1
SH.FMC_A1.2=FMC_A1,13b-sda2
SH.FMC_A1.ConfNb=3
SH.FMC_A10.0=FMC_A10,13b-a1
SH.FMC_A10.1=FMC_A10,13b-sda1
SH.FMC_A10.2=FMC_A10,13b-sda2
SH.FMC_A10.ConfNb=3
SH.FMC_A11.0=FMC_A11,13b-a1
SH.FMC_A11.1=FMC_A11,13b-sda1
SH.FMC_A11.2=FMC_A11,13b-sda2
SH.FMC_A11.ConfNb=3
SH.FMC_A12.0=FMC_A12,13b-a1
SH.FMC_A12.1=FMC_A12,13b-sda1
SH.FMC_A12.2=FMC_A12,13b-sda2
SH.FMC_A12.ConfNb=3
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.1=FMC_BA0,FourSdramBanks2
SH.FMC_A14_BA0.ConfNb=2
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.1=FMC_BA1,FourSdramBanks2
SH.FMC_A15_BA1.ConfNb=2
SH.FMC_A2.0=FMC_A2,13b-a1
SH.FMC_A2.1=FMC_A2,13b-sda1
SH.FMC_A2.2=FMC_A2,13b-sda2
SH.FMC_A2.ConfNb=3
SH.FMC_A3.0=FMC_A3,13b-a1
SH.FMC_A3.1=FMC_A3,13b-sda1
SH.FMC_A3.2=FMC_A3,13b-sda2
SH.FMC_A3.ConfNb=3
SH.FMC_A4.0=FMC_A4,13b-a1
SH.FMC_A4.1=FMC_A4,13b-sda1
SH.FMC_A4.2=FMC_A4,13b-sda2
SH.FMC_A4.ConfNb=3
SH.FMC_A5.0=FMC_A5,13b-a1
SH.FMC_A5.1=FMC_A5,13b-sda1
SH.FMC_A5.2=FMC_A5,13b-sda2
SH.FMC_A5.ConfNb=3
SH.FMC_A6.0=FMC_A6,13b-a1
SH.FMC_A6.1=FMC_A6,13b-sda1
SH.FMC_A6.2=FMC_A6,13b-sda2
SH.FMC_A6.ConfNb=3
SH.FMC_A7.0=FMC_A7,13b-a1
SH.FMC_A7.1=FMC_A7,13b-sda1
SH.FMC_A7.2=FMC_A7,13b-sda2
SH.FMC_A7.ConfNb=3
SH.FMC_A8.0=FMC_A8,13b-a1
SH.FMC_A8.1=FMC_A8,13b-sda1
SH.FMC_A8.2=FMC_A8,13b-sda2
SH.FMC_A8.ConfNb=3
SH.FMC_A9.0=FMC_A9,13b-a1
SH.FMC_A9.1=FMC_A9,13b-sda1
SH.FMC_A9.2=FMC_A9,13b-sda2
SH.FMC_A9.ConfNb=3
SH.FMC_D0_DA0.0=FMC_D0,16b-d1
SH.FMC_D0_DA0.1=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.2=FMC_D0,sd-16b-d2
SH.FMC_D0_DA0.ConfNb=3
SH.FMC_D10_DA10.0=FMC_D10,16b-d1
SH.FMC_D10_DA10.1=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.2=FMC_D10,sd-16b-d2
SH.FMC_D10_DA10.ConfNb=3
SH.FMC_D11_DA11.0=FMC_D11,16b-d1
SH.FMC_D11_DA11.1=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.2=FMC_D11,sd-16b-d2
SH.FMC_D11_DA11.ConfNb=3
SH.FMC_D12_DA12.0=FMC_D12,16b-d1
SH.FMC_D12_DA12.1=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.2=FMC_D12,sd-16b-d2
SH.FMC_D12_DA12.ConfNb=3
SH.FMC_D13_DA13.0=FMC_D13,16b-d1
SH.FMC_D13_DA13.1=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.2=FMC_D13,sd-16b-d2
SH.FMC_D13_DA13.ConfNb=3
SH.FMC_D14_DA14.0=FMC_D14,16b-d1
SH.FMC_D14_DA14.1=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.2=FMC_D14,sd-16b-d2
SH.FMC_D14_DA14.ConfNb=3
SH.FMC_D15_DA15.0=FMC_D15,16b-d1
SH.FMC_D15_DA15.1=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.2=FMC_D15,sd-16b-d2
SH.FMC_D15_DA15.ConfNb=3
SH.FMC_D1_DA1.0=FMC_D1,16b-d1
SH.FMC_D1_DA1.1=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.2=FMC_D1,sd-16b-d2
SH.FMC_D1_DA1.ConfNb=3
SH.FMC_D2_DA2.0=FMC_D2,16b-d1
SH.FMC_D2_DA2.1=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.2=FMC_D2,sd-16b-d2
SH.FMC_D2_DA2.ConfNb=3
SH.FMC_D3_DA3.0=FMC_D3,16b-d1
SH.FMC_D3_DA3.1=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.2=FMC_D3,sd-16b-d2
SH.FMC_D3_DA3.ConfNb=3
SH.FMC_D4_DA4.0=FMC_D4,16b-d1
SH.FMC_D4_DA4.1=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.2=FMC_D4,sd-16b-d2
SH.FMC_D4_DA4.ConfNb=3
SH.FMC_D5_DA5.0=FMC_D5,16b-d1
SH.FMC_D5_DA5.1=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.2=FMC_D5,sd-16b-d2
SH.FMC_D5_DA5.ConfNb=3
SH.FMC_D6_DA6.0=FMC_D6,16b-d1
SH.FMC_D6_DA6.1=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.2=FMC_D6,sd-16b-d2
SH.FMC_D6_DA6.ConfNb=3
SH.FMC_D7_DA7.0=FMC_D7,16b-d1
SH.FMC_D7_DA7.1=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.2=FMC_D7,sd-16b-d2
SH.FMC_D7_DA7.ConfNb=3
SH.FMC_D8_DA8.0=FMC_D8,16b-d1
SH.FMC_D8_DA8.1=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.2=FMC_D8,sd-16b-d2
SH.FMC_D8_DA8.ConfNb=3
SH.FMC_D9_DA9.0=FMC_D9,16b-d1
SH.FMC_D9_DA9.1=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.2=FMC_D9,sd-16b-d2
SH.FMC_D9_DA9.ConfNb=3
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.1=FMC_NBL0,Sd2ByteEnable2
SH.FMC_NBL0.ConfNb=2
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.1=FMC_NBL1,Sd2ByteEnable2
SH.FMC_NBL1.ConfNb=2
SH.FMC_NOE.0=FMC_NOE,Sram1
SH.FMC_NOE.ConfNb=1
SH.FMC_NWE.0=FMC_NWE,Sram1
SH.FMC_NWE.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,13b-sda1
SH.FMC_SDCLK.1=FMC_SDCLK,13b-sda2
SH.FMC_SDCLK.ConfNb=2
SH.FMC_SDNCAS.0=FMC_SDNCAS,13b-sda1
SH.FMC_SDNCAS.1=FMC_SDNCAS,13b-sda2
SH.FMC_SDNCAS.ConfNb=2
SH.FMC_SDNRAS.0=FMC_SDNRAS,13b-sda1
SH.FMC_SDNRAS.1=FMC_SDNRAS,13b-sda2
SH.FMC_SDNRAS.ConfNb=2
SH.FMC_SDNWE.0=FMC_SDNWE,13b-sda1
SH.FMC_SDNWE.1=FMC_SDNWE,13b-sda2
SH.FMC_SDNWE.ConfNb=2
SH.GPXTI15.0=GPIO_EXTI15
SH.GPXTI15.ConfNb=1
SH.GPXTI6.0=GPIO_EXTI6
SH.GPXTI6.ConfNb=1
SPI1.CalculateBaudRate=45.0 MBits/s
SPI1.Direction=SPI_DIRECTION_2LINES
SPI1.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate
SPI1.Mode=SPI_MODE_MASTER
SPI1.VirtualType=VM_MASTER
SPI2.CalculateBaudRate=22.5 MBits/s
SPI2.Direction=SPI_DIRECTION_2LINES
SPI2.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate
SPI2.Mode=SPI_MODE_MASTER
SPI2.VirtualType=VM_MASTER
SPI3.CalculateBaudRate=22.5 MBits/s
SPI3.Direction=SPI_DIRECTION_2LINES
SPI3.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate
SPI3.Mode=SPI_MODE_MASTER
SPI3.VirtualType=VM_MASTER
TIM10.IPParameters=Prescaler
TIM10.Prescaler=299
TIM11.IPParameters=Prescaler
TIM11.Prescaler=299
TIM12.IPParameters=Prescaler
TIM12.Prescaler=299
TIM13.IPParameters=Prescaler
TIM13.Prescaler=299
TIM14.IPParameters=Prescaler
TIM14.Prescaler=299
TIM8.IPParameters=Prescaler,Period
TIM8.Period=99
TIM8.Prescaler=179
TIM9.IPParameters=Prescaler
TIM9.Prescaler=299
USART1.IPParameters=VirtualMode
USART1.VirtualMode=VM_ASYNC
USART6.IPParameters=VirtualMode
USART6.VirtualMode=VM_ASYNC
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM10_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM10_VS_ClockSourceINT.Signal=TIM10_VS_ClockSourceINT
VP_TIM11_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM11_VS_ClockSourceINT.Signal=TIM11_VS_ClockSourceINT
VP_TIM12_VS_ClockSourceINT.Mode=Internal
VP_TIM12_VS_ClockSourceINT.Signal=TIM12_VS_ClockSourceINT
VP_TIM13_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM13_VS_ClockSourceINT.Signal=TIM13_VS_ClockSourceINT
VP_TIM14_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM14_VS_ClockSourceINT.Signal=TIM14_VS_ClockSourceINT
VP_TIM8_VS_ClockSourceINT.Mode=Internal
VP_TIM8_VS_ClockSourceINT.Signal=TIM8_VS_ClockSourceINT
VP_TIM9_VS_ClockSourceINT.Mode=Internal
VP_TIM9_VS_ClockSourceINT.Signal=TIM9_VS_ClockSourceINT
board=custom
isbadioc=false
